{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil3"],"not_rendered":{"macros":1},"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"merged":[[6,2,6,3],[6,6,6,7],[6,10,6,11],[6,14,6,15],[7,2,7,3],[7,6,7,7],[7,10,7,11],[7,14,7,15],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,36,2],[35,3,36,3],[35,4,36,4],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[43,2,43,3],[44,1,44,3],[50,1,50,3]]}
[]
[]
[null,"Cellule pilotante",3,null,"indique le nbre de pièces"]
[]
[]
[]
[null,"Nom :","Pièce mâle"]
[null,"Matière :","3 - Inconel 718"]
[null,"L",{"v":15,"d":"15.000"},"mm"]
[null,"Dext",{"v":73.42,"d":"73.420"},"mm"]
[null,"dint",{"v":58.85,"d":"58.850"},"mm"]
[null,"Diamètre de calcul",{"v":65,"d":"65.000"},"mm"]
[null,"Young Montage",{"v":206748.22,"d":"206748"},"daN/mm2"]
[null,"Youg MeF",218090,"daN/mm2"]
[null,"Young fonctionnement",218090,"daN/mm2"]
[null,"S",{"v":523.7919958312035,"d":"523.792"},"mm2",null,"Tableau à dupliquer x-1 fois. Le nombre total doit être égal au nombre de pièces"]
[null,"Kv (montage)",{"v":7219537.5192232495,"d":"7.220E+06"},"daN/mm"]
[null,"Kv (MeF)",{"v":7615586.424721811,"d":"7.616E+06"},"daN/mm"]
[null,"Kv (fonctionnement)",{"v":7615586.424721811,"d":"7.616E+06"},"daN/mm"]
[null,"ΔL/L MeF",{"v":11.804804,"d":"11.805"},"*10^-5"]
[null,"ΔL/L Fonctionnement",{"v":9.6756,"d":"9.676"},"*10^-5"]
[null,"ν",{"v":0.2795269411764706,"d":"0.28"},"-"]
[null,"ρ",8260,"kg/m3"]
[null,"Frettage en def",170,"microns"]
[]
[]
[]
[]
[]
[null,"Vitesse de rotation",null,30000,"tr/min"]
[{"$nulls":3},{"v":3141.592,"d":"3142"},"rad/s"]
[null,"Pression intérieure mâle",null,{"v":10,"d":"10.0"},"bar"]
[null,"Pression extérieure mâle",null,{"v":20,"d":"20.0"},"bar"]
[null,"Pression intérieure femelle",null,{"v":20,"d":"20.0"},"bar"]
[null,"Pression extérieure femelle",null,{"v":10,"d":"10.0"},"bar",null,"Tableau invariant"]
[null,"Effort axial F (traction F=+..., compression F=-...)",null,6000,"daN"]
[]
[null,"Température Montage",null,293,"K"]
[null,"Température Mise en froid",null,70,"K"]
[null,"Température Fonctionnement",null,70,"K"]
[null,"Coefficient de frottement",null,0.12,"-"]
[]
[]
[null,"Nom :","Pièce mâle"]
[null,"Au niveau du frettage"]
[null,"Contrainte axiale",{"v":39.64062230404313,"d":"39.64"},"MPa"]
[null,"Contrainte radiale",{"v":-32.33516059093657,"d":"-32.34"},"MPa"]
[null,"Contrainte tangentielle",{"v":-148.55413721334097,"d":"-148.55"},"MPa"]
[null,"Déformée axiale",{"v":2.8760070319379144E-3,"d":"0.003"},"mm"]
[null,"Déformée radiale",{"v":-0.0477975216622523,"d":"-0.048"},"mm",null,"Tableau à dupliquer x-1 fois. Le nombre total doit être égal au nombre de pièces"]
[null,"Dans la pièce, au diamètre particulier"]
[null,"Contrainte axiale",{"v":39.64062230404313,"d":"39.64"},"MPa"]
[null,"Contrainte radiale",{"v":-16.305243565481362,"d":"-16.31"},"MPa"]
[null,"Contrainte tangentielle",{"v":-164.58405423879614,"d":"-164.58"},"MPa"]
[null,"Déformée axiale",{"v":2.8760070319379144E-3,"d":"0.003"},"mm"]
[null,"Déformée radiale",{"v":-0.05379465846487457,"d":"-0.054"},"mm"]

{"sheet":"Feuil2","index":1,"n_rows":24,"n_cols":6,"rows_kept":24,"merged":[[3,2,3,3],[4,1,4,3],[5,1,5,3],[6,1,6,3],[14,1,14,3],[15,1,15,3],[16,1,16,3]]}
[]
[]
[]
[null,"Nom :","Pièce mâle"]
[]
[null,"Effet de la centrifugation seule"]
[null,"Au niveau du frettage"]
[null,"Contrainte radiale",{"v":0,"d":"0.00"},"MPa"]
[null,"Contrainte tangentielle",{"v":77.65956330299065,"d":"77.66"},"MPa"]
[null,"Déformée radiale",{"v":0.02614409252008608,"d":"0.026"},"mm au diamètre"]
[null,"Dans la pièce, au diamètre particulier",{"v":65,"d":"65.00"},"mm"]
[null,"Contrainte radiale",{"v":1.7554812146867698,"d":"1.76"},"MPa"]
[null,"Contrainte tangentielle",{"v":91.10080679126315,"d":"91.10"},"MPa",null,"Tableau à dupliquer x-1 fois. Le nombre total doit être égal au nombre de pièces"]
[null,"Déformée radiale",{"v":0.027005624569246118,"d":"0.027"},"mm au diamètre"]
[]
[null,"Effet de la pression seule"]
[null,"Au niveau du frettage"]
[null,"Contrainte radiale",{"v":-2,"d":"-2.00"},"MPa"]
[null,"Contrainte tangentielle",{"v":-5.594198219475679,"d":"-5.59"},"MPa"]
[null,"Déformée radiale",{"v":-1.6950813757235607E-3,"d":"-0.002"},"mm au diamètre"]
[null,"Dans la pièce, au diamètre particulier",{"v":65,"d":"65.00"},"mm"]
[null,"Contrainte radiale",{"v":-1.5042573863094295,"d":"-1.50"},"MPa"]
[null,"Contrainte tangentielle",{"v":-6.089940833166249,"d":"-6.09"},"MPa"]
[null,"Déformée radiale",{"v":-1.68973783240813E-3,"d":"-0.002"},"mm au diamètre"]

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}